Construction of Prusa i3 by 3kd

Notes

Tips and tricks for 3D printing:

Tips and tricks on perparing complex models for 3D printing

Top 10 Tips for 3D Printing Design

Prototypes That Last: Simple Tips for Making Durable Parts, Part 1

Prototypes That Last: Simple Tips for Making Durable Parts, Part 2

Resin Casting: Going from CAD to Engineering-Grade Plastic Parts

10 Tips For Modeling For 3D Printing

Material

Extruder: 0.4mm or 400 micron
(Warning: When buying metal extru itders. If there is no teflon tube inside, it will not work with PLA. It blocks when hot)

Configuration of Slic3r

Layer height: never go over 80% of the extruder hardware value.

Shops

http://reprap.me/